

Fig.3: Dielectric constant (ε) as a function of temperature (T) at different frequencies (103-2.106Hz) for ilmenite CdTiO3 ceramics.